**Made to Measure Track Order Form**

**Part 1 of 2**

*(If ordering a bent track, please also complete part 2 “Bay window measurements”)*

**\*IN ORDER TO CONFIRM TO BS EN 13120 CHILD SAFEY LEGISLATION:**

*Installation height – in order to conform to child safety legislation; your chain drop must be at least 150cm less than your installation height (i.e the bottom of the cord must be 1.5m from the floor) & fixed in safety device to the wall.*

**IMPORTANT INFORMATION**

**CORDED TRACKS**

We are required by law to ask for the height of installation, so that we can ensure the bottom of the cord loop we supply is a minimum of 150cm from the floor. If you do not know your installation height specify “unknown”, we will supply your track with a cord drop of 100cm – We recommend discussing this with your fitter prior to placing your order, as they may be required by law to shorten the cord in order to conform to BS EN 13120 child safety legislation.

**Any additional information:**

|  |  |
| --- | --- |
| **Account Number:**  | ***Date:*** |
|  **Account Name:****Your order reference:** |
| **Delivery Address:** *(If left blank we will assume that delivery is to your standard delivery address)* | ***Postcode:*** |

**DID YOU KNOW?**

You can get a quote and place your made to measure track order online via Webtex: [www.evans-textiles.com](http://www.evans-textiles.com) : We will then ask you relevant questions, making your ordering process easier and giving you confidence in complying with the legislation. Best of all you receive a **10%** discount when ordering via Webtex!

|  |  |
| --- | --- |
| ***ALL TRACKS*** | ***CORDED TRACK ONLY/ EVAGLIDE*** |
| ***QTY*** | ***SYSTEM*** | ***COLOUR*** | ***LENGTH*** *(cm)* | ***STRAIGHT OR BENT***  | ***BRACKETS*** *(top or face fix which project on brackets)* | ***GLIDER TYPE & COLOUR (white, black & silver)*** | ***STACK*** *(PAIR, LH, RH)* | ***ORDER REF*** | ***INSTALLTION*** *(height)* | ***CORD DROP*** *(cm)* | ***CORD SIDE*** *(cm)* | ***CORD COLOUR*** *(black, white & silver)* | ***FINIAL TYPE*** | ***ADD OR INCLUDE FINIALS WITHIN THE LENGTH (Track size is ‘I’ for including finials or ‘E’ for excluding finials*** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |